|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Buffer** | | | | |
| **Equipment** | **Information and Function** | **Quantity** | **Size in m** | **Photo** |
| 3000 L Jacketed Cubital Tank with Load Cell | extremely flexible, modular mixing system that reproducible single-use mixing | 1 | 1.64 x 1.40 x 3.56 | 3000 L Jacketed Cubital Tank with Load Cell |
| 2000 L Jacketed Cubical Tank with Load Cell | extremely flexible, modular mixing system that reproducible single-use mixing | 2 | 1.78 x 1.39 x 2.65 | 2000 L Jacketed Cubical Tank with Load Cell |
| 1500 L Jacketed Cubical Tank with Load Cell | extremely flexible, modular mixing system that reproducible single-use mixing | 3 | 1.62 x 1.39 x 2.17 | 1500 L Jacketed Cubical Tank with Load Cell |
| 1000 L Jacketed Cubical Tank with Load Cell | extremely flexible, modular mixing system that reproducible single-use mixing | 3 | 1.53 x 1.29 x 1.60 | 1000 L Jacketed Cubical Tank with Load Cell |
| 500 L formulation tank | Formulation | 4 | 0.72 x 0.83 x 1.39 | Formulation tank |
| 400 L Jacketed Cubical Tank with Load Cell | extremely flexible, modular mixing system that reproducible single-use mixing | 5 | 1.27 x 1.01 x 1.58 | 400 L Jacketed Cubical Tank with Load Cell |
| 200 L stainless steel Bioreactor with Trolley | extremely flexible, modular mixing system that reproducible single-use mixing | 3 | 0.82 x 0.65 x 1.2 |  |
| 100 L stainless steel Tank | extremely flexible, modular mixing system that reproducible single-use mixing | 3 | 1.00 x 0.86 x 1.58 |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Buffer** | | | | |
| **Equipment** | **Information and Function** | **Quantity** | **Size in m** | **Photo** |
| 3000 L Jacketed Cubital Tank with Load Cell | extremely flexible, modular mixing system that reproducible single-use mixing | 1 | 1.64 x 1.40 x 3.56 | 3000 L Jacketed Cubital Tank with Load Cell |
| 1000 L Jacketed Cubical Tank with Load Cell | extremely flexible, modular mixing system that reproducible single-use mixing | 1 | 1.53 x 1.29 x 1.60 | 1000 L Jacketed Cubical Tank with Load Cell |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Media and feed storage and preparation room** | | | | |
| **Equipment** | **Information and Function** | **Quantity** | **Size in m** | **Photo** |
| 2000 L Jacketed Cubical Tank with Load Cell | extremely flexible, modular mixing system that reproducible single-use mixing | 3 | 1.78 x 1.39 x 2.65 | 2000 L Jacketed Cubical Tank with Load Cell |
| 200 L stainless steel Bioreactor with Trolley | extremely flexible, modular mixing system that reproducible single-use mixing | 1 | 0.82 x 0.65 x 1.2 |  |
| 2 x 20 L Biocontainers with Trolley | For single-use bio containers | 1 | 0.71x1.05x0.98 | Ein Bild, das Vervielfältiger enthält.  Automatisch generierte Beschreibung |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 500 L formulation tank | Formulation of feed | 3 | 0.72 x 0.83 x 1.39 | Formulation tank |
| 100 L Jacketed Cubical Tank with Load Cell, Stainless Steel | extremely flexible, modular mixing system that provides reproducible single-use mixing | 1 | 1 x 0.86 x 1.58 | Ein Bild, das Tisch enthält.  Automatisch generierte Beschreibung |